**CALBO**

**ACCESSIBILITY CONSTRUCTION INSPECTION CHECKLIST**

*The CALBO Access Committee in collaboration with the California Commission on Disability Access (CCDA) checklist committee is pleased to provide this Accessibility Checklist for use by building inspectors as a supplemental tool to assist with on-site inspection of accessibility features and construction elements affecting accessibility compliance. This checklist is based on the 2013 California Building Code (CBC), Part 2, Title 24, California Code of Regulations and should be used in conjunction with the regulations found in Chapter 11B of the CBC.*

*The purpose of this checklist is to provide building inspectors with a tickler style checklist of the most common accessibility features to be inspected and/or verified during the construction phases of commercial projects. It is important during the progress inspections that the building inspector verify all elements will be able to meet the minimum accessibility requirements of the California Building Code at the time of final inspection. This checklist represents a guide for the building inspector and is not intended to be a complete list for full access compliance or to identify any specific measurements or detailed requirements. This checklist is intended for use by trained building code officials.*

*The building inspector must assess the elevations and slopes of the existing streets and sidewalks, location of existing buildings, existing drainage and other physical conditions of the property relative to the accessibility improvements on the proposed plans. During construction inspection finish product thicknesses such as flooring materials or wall coverings must be considered when reviewing critical accessibility features, including but not limited to, widths of halls, corridors, door strike side, plumbing locations, built-in cabinets, and shower compartments.*

|  |  |
| --- | --- |
| **ROUGH GRADE SITE INSPECTION** | |
| Locate and verify the plan specified accessible routes from existing public sidewalks, accessible parking locations, and other site arrival points to building entrances and exits. | 11B-206.1 |
| Identify the plan specified accessible routes from all entrances and exits to common and public use areas on the site. | 11B-206.2.2 |
| If site conditions have swamp type lands, steep grades, drainage ditches, flood hazards or other inconsistencies with the approved plans, proper methods of compliance shall be reviewed and approved by the building official/plan checker prior to continuing. |  |
| Verify that drainage, drainage swales, catch basins and grates do not violate slope or surface requirements along accessible routes, accessible parking and access aisles, etc. | 11B-403 |
| Verify if under-slab plumbing will provide adequate clearances from finished walls. |  |
| Site Lighting shall be capable of providing a minimum of one foot candle to the surface. | 1006 |
| **ROUGH FORM AND FOUNDATION INSPECTION** | |
| Verify building form elevations are set relative to site features (accessible routes, accessible parking, common and public use areas, and other site arrival points) to ensure correct accessible slopes (5% running slope and 2.08% cross slope). | 11B-403 |
| Verify forms for sidewalks, ramps, landings, curb ramps and clear floor spaces are correctly installed so proper slopes, cross slopes, widths and clearances will be maintained at final inspection. | 11B, Division 4 Accessible Routes. |
| Verify no abrupt changes in level will exceed ½” in the path of travel or 4” drop offs along edges. | 11B-303.5 |
| Verify forms include guardrail and handrail sleeves if required. | 11B-505 |
| Verify planned site lighting sleeves are provided. | 1006 |

|  |  |
| --- | --- |
| **ROUGHS/FOUR WAY INSPECTION CHECKLIST** | |
| **VERIFY FRAMING – remember finish material thicknesses!** |  | |
| Slope, width and headroom of all interior accessible routes. | 11B-402 | |
| Door opening widths. | 11B-404 | |
| Maneuvering clearances/landings at doors. | 11B-404 | |
| Distance between doors in series. | 11B-404.2.6 | |
| Grab bar backing in toilet/shower rooms. | 11B-604.5,  11B-607.4, 11B-608.3 | |
| Backing for grab bars in bathtub/shower rooms. | 11B-610 | |
| Width and depth of shower stalls. | 11B-608.2 | |
| Drinking fountain alcoves/wing walls. | 11B-602.9 | |
| Tread dimensions on stairs including nosings. Verify finish materials for variances | 11B-504 | |
| Backing for handrails at ramps/stairs. | 11B-505 | |
| Elevator shaft dimensions. Check plans for Fire Assembly thickness | 11B-407.4 | |
| Location of controls for operable windows to meet reach range and operation | 11B-229 | |
| Restroom dimensions. | 11B-604.8 | |
| **VERIFY ELECTRICAL – remember finish material thicknesses!** |  | |
| Heights of all 30 amp or less outlet boxes. Measure to top or bottom of boxes | 11B-308.1.1 | |
| Heights of all electrical switch boxes. Measure to top or bottom of boxes | 11B-308.1.2 | |
| Alarm/detector systems. | 11B-702 | |
| Height of HVAC controls. | 11B-308 | |
| Location of elevator control/call/notification boxes. | 11B-407 | |
| Installation of emergency egress lighting if required. High and Low | 11B-1011 | |
| **VERIFY ROUGH PLUMBING – remember finish material thicknesses!** |  | |
| Location of toilet flanges from walls. | 11B-604.2 | |
| Location of lavatory traps from side walls. | 11B-606.6 | |
| Location of bathtub controls and drain. | 11B-607.5 | |
| Installation height and location of shower controls. | 11B-608.5 | |
| Location of shower drains and floor slope. | 11B-608.5 | |
| Shower threshold. | 11B-608.7 | |
| Kitchen or Common use sink plumbing | 11B-608.5  11B-804 | |
| Plumbing for Drinking Fountains. Both high and low | 11B-602 | |

|  |  |
| --- | --- |
| **(OPTIONAL INSPECTION Pre-Concrete/Asphalt)** Exterior Site sidewalk forms and grading per page 1 | |
| **FINAL INSPECTION CHECKLIST** | |
| **EXTERIOR ROUTES** |  |
| Floor and ground surfaces stable, firm and slip resistant. | 11B-302.1 |
| Openings in floor or ground surfaces 1/2 inch maximum with long dimension perpendicular to direction of travel. | 11B-302.3 |
| Vertical change in level 1/4 inch high maximum. | 11B-303.2 |
| Changes in level greater than 1/2 inch ramped. | 11B-303.4 |
| Abrupt changes in level exceeding 4 inches, vertical dimension shall be identified by warning curb. | 11B-303.5 |
| Running and cross slopes at walking surfaces. Walks, sidewalks and ramps. | 11B-403.3  11B-405 |
| Vertical clearances/protrusions along circulation paths. | 11B-307 |
| Site arrival points. An accessible route from parking, passenger loading zones, public streets and sidewalks to building entrance or facility. | 11B-206.2.1 |
| Within a site. One accessible route connecting accessible buildings, accessible facilities, accessible elements, and accessible spaces. | 11B-206.2.2 |
| Location of accessible routes coincides with general circulation paths. | 11B-206.2.1 Exception 3 |
| Clear width of walking surface. | 11B-403.5.1 |
| Contrasting stripe on upper approach and all treads. | 11B-504.4.1 |
| No open risers on stairways. | 11B-504.3 |
| Handrails on ramps and stairways. | 11B-505 |
| Curb ramps, blended transitions and islands. | 11B-406 |
| Raised islands in crossings shall be cut through level with the street or have curb ramps at both sides. | 11B-406.6 |
| Installation and color of required detectable warnings. | 11B-705 |
| Passing spaces along accessible routes with a clear width less than 60 inches. | 11B-403.5.3 |
| Walks with continuous gradients have resting areas. | 11B-403.7 |
| **INTERIOR ROUTES** |  |
| Floor and ground surfaces stable, firm and slip resistant. | 11B-302.1 |
| Carpet pile height 1/2 inch maximum. Exposed edges securely fastened with trim on exposed edge. | 11B-302.2 |
| Vertical clearances/protrusions along circulation paths. | 11B-307 |
| Running and cross slopes at walking surfaces and ramps. | 11B-403.3  11B-405 |
| Handrails on ramps and stairways. | 11B-505 |
| Vertical change in level 1/4 inch high maximum. | 11B-303.2 |
| Changes in level greater than 1/2 inch ramped. | 11B-303.4 |
| Contrasting stripe at upper approach and lower tread. | 11B-504.4.1 |
| Accessible route to all functional areas of restaurants and dining facilities. | 11B-206.2.5 |
| Accessible route to performance area from an assembly area. | 11B-206.2.6 |
| Common use circulation paths within employee work areas. | 11B-206.2.8 |
| Accessible route to both sides of court sports. | 11B-206.2.12 |
| Clear width of walking surfaces. | 11B-403.5.1 |
| Width of accessible route at 180 degree turns. | 11B-403.5.2 |
| **PARKING** |  |
| Location and number of van parking and standard parking spaces. | 11B-208 |

|  |  |
| --- | --- |
| Dimensions of accessible parking spaces and access aisles. | 11B-502.2  11B-502.3 |
| Marking at access aisles. | 11B-502.3.3 |
| Slope of accessible parking spaces and access aisles. | 11B-502.4 |
| Identification at accessible spaces and/or lot entrances. | 11B-502.6  11B-502.8 |
| Vertical clearance at parking spaces, access aisles and vehicular routes. | 11B-502.5 |
| Location, number and dimensions of passenger drop-off zones. | 11B-503 |
| Vertical clearance at vehicle pull-up spaces, access aisle, vehicular route. | 11B-503.5 |
| Passenger loading zone, accessible parking spaces and access aisles in valet lots. | 11B-209.4 |

|  |  |
| --- | --- |
| **REACH RANGES** **AND OPERABLE PARTS** |  |
| Forward and side reach | 11B-308.2/3 |
| Over projections | 11B-308.2.2/3.2 |
| Clear floor space at controls | 11B-309.2 |
| 5lbs operating force | 11B-309.4 |
| Reach ranges | 11B-309.3 |
| No tight grasping, pinching, twisting of wrist | 11B-309.4 |
| Top and bottom of switches and outlets AFF | 11B-308.1.1&2 |
| **DOORS** |  |
| 32” clear width | 11B-404.2.3 |
| Maneuvering clearances | 11B-404.2.4.1 |
| Level landings each side of doors | 11B-404.2.4.4 |
| Thresholds | 11B-404.2.5 |
| Doors in series | 11B-404.2.6 |
| Hardware | 11B-404.2.7 |
| Closing speed | 11B-404.2.8.1 |
| 5lbs opening force | 11B-404.2.9 |
| 10” smooth surface on push side of door | 11B-404.2.10 |
| Signs – Tactile/Braille | 11B-703 |
| **VERTICAL ACCESS** |  |
| Elevators: Controls; visual and audio signals | 11B-407.2 |
| Elevators: Symbols | 11B-407.4.7.1 |
| Elevators: Support rail | 11B-407.4.10 |
| Platform Lifts | 11B-410 |
| Destination-oriented Elevators (July 2015) | 11B-411 |
| Stairs | 11B-504 |
| **PLUMBING/RESTROOMS** |  |
| Turning space within the room | 11B-603 |
| Door swing not in clear floor space of any fixture (except single-user) | 11B-603 |
| Mirrors and accessories | 11B-603 |
| Clear floor space requirements at fixtures | 11B-604 |
| Compartment configuration side and end entry, toe clearances | 11B-604 |
| Side and rear wall grab bars | 11B-609 |
| Ambulatory compartments | 11B-604.8.2 |
| Urinals | 11B-605 |
| Accessible lavatories, heights, knee clearances | 11B-606 |
| Restroom symbols on door | 11B-703.7.2.6 |
| Shower compartments | 11B-608 |
| Bathtubs | 11B-607 |
| Drinking fountains | 11B-211, 11B-602 |
| **BUILT-IN ELEMENTS** |  |
| Dining/work surfaces | 11B-226, 11B-902.2 |
| Benches | 11B-903.2 |
| Check out aisles | 11B-904.3.2 |
| Sales/service counters | 11B-227, 11B-904.4.1 |
| Food service lines | 11B-904.5.1 |
| Accessible sinks | 11B-212, 11B-606 |
| **MISCELLANEOUS ELEMENTS** |  |
| Fire alarm systems: visible alarms | 11B-215, 11B-702 |
| Assistive Listening Systems | 11B-219, 11B-706 |
| ATMs, POS Machines, Fare Machines | 11B-220, 11B-707 |
| Windows | 11B-229 |
| Exercise Machines and Equipment | 11B-236 |
| Dressing, Fitting, and Locker Rooms | 11B-222 |
| Assembly areas: companion seats; wheelchair seats; semi-ambulant seats | 11B-221, 11B-802 |
| Storage | 11B-225, 11B-811 |
| Signs | 11B-216, 11B-703 |
| Variable Message Systems (July 2015) | 11B-703.8 |
| Exit Signs | 1007.6 |
| Areas of Rescue | Chapter 10 |
| Telephones and TTYs | 11B-217, 11B-704 |
| Vending Machines, Mail Boxes, Change Machines | 11B-228 |
| Play Areas | 11B-240, 11B-1008 |
| Swimming Pools, Wading Pools, and Spas | 11B-242, 11B-1009 |
| Sauna and Steam Rooms | 11B-241, 11B-612 |

*Please note that this is not an exhaustive list of the elements and spaces required to be accessible per the 2013 California Building Code. Items included to be inspected for compliance if provided, including but not limited to: outdoor developed areas, bus shelters, amusement rides, recreational boating facilities, fishing piers and platforms, golf and miniature golf facilities, and shooting facilities with firing positions.*